miim

### Options in the DOWNL.OAD File

#### Convert from DCC to Manual

To convert a DCC DOWNL.OAD file to a joystick manual Excel CMM, you must change the following lines:

- Line S25X1Y1Z1W0U9 - This line controls the presence of a PH9. To change to no PH9, change the line to: S25X1Y1Z1W0U0

- Line S1XvalueYvalueZvalueWvalue - This line controls the speed of the CMM. To convert to manual, change the line to: S1X0Y0Z0W0

- Line S2Qvalue - This line controls the acceleration of the CMM. To convert to manual, change the line to: S2Q0

#### Reversing Jog Box Polarity for One or More Axes

Line S1DX0Y0Z0 - This line controls whether the motion of the axes adheres to the normal convention on the jog box or is opposite to the normal convention when the input specifies reversed polarity. A value of 0 means that it uses the normal convention.

To reverse the polarity, use a value of FF.

To reverse the polarity for the Z axis only, the line would be: S1DX0Y0ZFF