miim

### MP-151 D/A updates were late or missing

On an MP-35, the MP has not sent the DCC board new axis position coordinates in the last 32 milliseconds. The digital/analog (D/A) board failed.

On an SMP-400, the servo D/A's have not been updated for at least 8 milliseconds.

For more information, see "DCC Error Codes".

What you should do:

1. To clear the error, power the MP down.

2. Power the MP back up.

3. If the error reoccurs, contact your Giddings & Lewis service representative.