settingseditor

### ACR2_MeasuredOrigin

This registry entry provides the XYZ offset in mm that is used during calibration of an ACR2 probe changer. It establishes the origin for an ACR2 port after measuring the location of the pin inside the port. Normally, you don't need to modify this registry entry.

Entry Name: ACR2_MeasuredOrigin

Entry Type: Character string that specifies the probe changer origin. The default value is "113.55 14.5 -31.5".