miim

### Updates

Version | Date | Who | Changes
1.254 | 08/02/06 | DS | Fixed problem of measurement in inches.
1.253 | 07/26/06 | DS | Implemented aiming to first hit of feature; also, replaced the use of MS_SELECT_REFLECTOR to m_ChangingDevice (was causing a problem in some cases); disabled double-click on ADM setup screen.
1.252 | 07/25/06 | DS | Allow motor off when beam is not locked (PR 242087), fixed problem of readout window not showing 'busy" state (PR 242030), display command error even when executed as TCU command (242027).
1.251 | 07/21/06 | DS | Fixed problem of OnErrorAnswer causing indefinite error messages; mapped error status to strings; fixed problem of some errors not displayed.
1.25 | 07/07/06 | DS | Resume scanning after broken beam, illegal file name (replace '.' with '_', nivel calculation (sign reversed and checked with Markus), do not correct level plain with level reset, disable nivel checking after nivel system error, fix the problem of infinite error messages (do not call PCDMessageBox in from the comm. thread), miscellaneous internal checks/changes.