Collapse All Expand All

PC-DMIS 2019 R1 Object Library |
SetScanParams Method
See Also Send Topic Feedback | See Object Hierarchy Chart

incr
  Increment value for LINE, BODY, and CUTAXIS scan techniques. Optional.

AXIS
  Axis for BODY and CUTAXIS scan techniques. PCD_XAXIS, PCD_YAXIS, PCD_ZAXIS. Optional.

max_incr
  For VARIABLE scan techniques. Optional.

min_incr
  For VARIABLE scan techniques. Optional.

MAX_ANGLE
  For VARIABLE scan techniques. Optional.

MIN_ANGLE
  For VARIABLE scan techniques. Optional.

delta
  Distance delta for FIXED_DELTA scans, time delta for VARIABLE_DELTA and TIME_DELTA scans. Optional.

DISTANCE
  Drop point distance for VARIABLE_DELTA scan, distance for CUTAXIS scan. Optional.

incr2
  Increment value in second direction for a patch scan. Optional.

axis2
  Second axis value for a patch scan (BODY scan technique only). Optional.

surf_thickness
  Surface thickness used to offset centroid calculation if necessary. Optional.

PCDLRN ActiveX DLL > OldBasic Object : SetScanParams Method

Glossary Item Box

# Description

Sets scan parameters (used in StartScan block)

# Syntax

Visual Basic
    Public Sub SetScanParams( _
       ByVal incr As Double, _
       ByVal AXIS As PAXISTYPE, _
       ByVal max_incr As Double, _
       ByVal min_incr As Double, _
       ByVal MAX_ANGLE As Double, _
       ByVal MIN_ANGLE As Double, _
       ByVal delta As Double, _
       ByVal DISTANCE As Double, _
       ByVal incr2 As Double, _
       ByVal axis2 As PAXISTYPE, _
       ByVal surf_thickness As Double _
    )

# Parameters

incr
  Increment value for LINE, BODY, and CUTAXIS scan techniques. Optional.
AXIS

  Value | Description
  --- | ---
  PCD_XAXIS | Mirrors the virtual machine's X axis.
  PCD_YAXIS | Mirrors the virtual machine's Y axis.
  PCD_ZAXIS | Mirrors the virtual machine's Z axis.

  Axis for BODY and CUTAXIS scan techniques. PCD_XAXIS, PCD_YAXIS, PCD_ZAXIS. Optional.
max_incr
  For VARIABLE scan techniques. Optional.
min_incr
  For VARIABLE scan techniques. Optional.
MAX_ANGLE
  For VARIABLE scan techniques. Optional.
MIN_ANGLE
  For VARIABLE scan techniques. Optional.
delta
  Distance delta for FIXED_DELTA scans, time delta for VARIABLE_DELTA and TIME_DELTA scans. Optional.
DISTANCE
  Drop point distance for VARIABLE_DELTA scan, distance for CUTAXIS scan. Optional.
incr2
  Increment value in second direction for a patch scan. Optional.
axis2

  Value | Description
  --- | ---
  PCD_XAXIS | Mirrors the virtual machine's X axis.
  PCD_YAXIS | Mirrors the virtual machine's Y axis.
  PCD_ZAXIS | Mirrors the virtual machine's Z axis.

  Second axis value for a patch scan (BODY scan technique only). Optional.
surf_thickness
  Surface thickness used to offset centroid calculation if necessary. Optional.

# See Also

OldBasic Object | OldBasic Members

Copyright © 2019. Hexagon Manufacturing Intelligence – Metrology Software, Inc. All Rights Reserved.