portable

## Leica Tracker Interface

The parameters that control how PC-DMIS interfaces with the Leica interface can be configured by selecting the Edit | Preferences | Machine Interface Setup menu item. This opens the Machine Options dialog box. The following tabs are available:

- Options tab

- Reset tab

- Sensor Configuration tab

- Environmental Parameters tab

- Level To Gravity tab

- System Information tab - Displays information for your configured Leica system. Included values are: IP Address, Tracker Type with Serial # (if available), Controller Type, T-CAM Type and Serial # (if available), emScon version, TP-Firmware version, Bootdriver version, and Nivel Type and Serial # (if available).

- Debug tab - For information, see the "Generating a Debug File" topic in the "Setting Your Preferences" chapter in the PC-DMIS Core documentation.

The Machine Interface Installation Manual (MIIM) provides additional information for this interface.

You can access the MIIM help file from this link: .

Minimum continuous scanning time and distance settings enforced by PC-DMIS

Tracker | Minimum Time | Minimum Distance
Leica (AT403) | 20ms (0.02) | -
Leica (AT901) | 100ms (0.1) | -
LeicaLMF (AT9x0) | 1ms (0.001) A performance hit occurs when setting a minimum time value less than 0.01 mm as Time Delta. | 0.01 mm You need to set the 403 min / max settings for 10Hz (901 is 1000 Hz).

For Leica AT9x0 trackers, if you lose communication between PC-DMIS and your AT9x0 tracker, the software displays a Connection Lost message and PC-DMIS goes into a "disconnected" state. Check your cabling or wifi to re-establish communication. Once you re-establish the communication, PC-DMIS returns to Online mode without restarting.