cmm

#### Tips to Use if None Explicitly Selected

Tips to use if none explicitly selected area

Use this area to specify the action that PC-DMIS should take if you did not explicitly select any probe tips in the Active tip list in the Probe Utilities dialog box prior to starting calibration.

If you explicitly choose tips in the Probe Utilities dialog box, only the selected tips are used.

- All - PC-DMIS uses all existing probe tip angles in the current probe file.

- Used in Routine - PC-DMIS only uses the probe tip angles that are used in the current measurement routine for the current probe file. The restrictions are as follows:

- - This option may not achieve the desired result if you use it in a measurement routine for which the Automatically Adjust Probe Head Wrist option is enabled. The tips used in the measurement routine at the time of the calibration may change later as a result of the actual part alignment.

  - This option looks only at the measurement routine that is currently open. It does NOT try to look through references to external files, such as subroutines.

- Abort execution - PC-DMIS aborts the execution or measurement. It treats the condition of no tip angles selected as an error condition.

These options do not apply to all operation types and all hardware types. Mainly, it is used with the "Calibrate Tips" or "Qualification Check" operation when used with a fixed head, indexing wrist, or infinite wrist if used in an indexing (non-mapped) mode.