settingseditor

### DccXYZ_1

Provides the default "Y" or "A" (angle) value for the center location for all auto features except a line where it defines the start point. The value will represent Y value when the "Cartesian" value is set to TRUE (1), and A when it is set to FALSE (0). This value and the "DccXYZ_0" and "DccXYZ_2" values are used for Contact probes while the "Point1(XYZ)" values are used for Vision and Laser probes.

Entry Name: DccXYZ_1

Entry Type: Real Number to specify the Y or A value. The default value is 0.