core

### Automatic Insertion of Temperature Compensation Command

For many types of machines, PC-DMIS automatically inserts the TEMPCOMP temperature compensation command when you create a measurement routine. This provides you with the opportunity to set up a measurement routine for temperature compensation. The Temperature Compensation dialog box appears, and you need to select the material of the part.

If you want PC-DMIS to automatically insert the temperature compensation command into a new measurement routine, select the Auto Insert Temperature Compensation in New Routine check box on the General tab in the Setup Options dialog box (Edit | Preferences | Setup).

If you do not want PC-DMIS to automatically insert the temperature compensation command into a new measurement routine, clear this check box.

PC-DMIS does not automatically insert the temperature compensation command into a new measurement routine for the following items:

- PC-DMIS NC software application

- PC-DMIS Planner software application

- Dual-arm CMMs

- Portable equipment

- Non-Hexagon controllers

- Machines with controllers that do not support temperature sensors