core

Step 3 - Define the Number of Ports

The final step prior to rack calibration of the Travel Rack HR-X1-TR is to define the quantity of ports on the rack you are calibrating.

To define the number of ports:

1. Select the Ports tab in the Probe Changer dialog box (Edit | Preferences | Probe Changer):

Probe Changer dialog box - Ports tab

2. In the Active probe changer list, select TYPE=TRAVELRACKX1V.

3. In the Number of ports box, type the number of ports the probe changer has.

4. To save your changes, click Apply.

The next step starts the calibration process.