portable

### Other PC-DMIS Menu Items

Operation Menu

End Feature (END) - Tells PC-DMIS that the number of hits for the feature has been reached and it can calculate the feature.

Erase Hit (Alt + -) - Deletes the last-measured hit.

Take Hit (Ctrl + H) - Measures a stationary T-Probe or Reflector position based on the measuring profile specified on the Sensor Configuration tab of the Machine Options dialog box or on the Tracker Operations toolbar, respectively.

Move To - Opens the Move Point dialog box, which enables you to insert a MOVE/POINT command into the measurement routine. See the "Inserting a Move Point Command" topic in the "Inserting Move Commands" chapter in the PC-DMIS Core documentation for more information.

Start/Stop Continuous Mode (Ctrl + I) - Starts or stops a scan, based on the basic scan settings on the Probing tab of the Parameter Settings dialog box (Edit | Preferences | Parameters). The default value for Distance delta provides a continuous distance separation of 2mm.

The AT401 does not support the Start/Stop Continuous Mode.