nc

### Step 1: Install the Probe and Macros

Use your probe system documentation to:

1. Install your probing system.

2. Install the probing macros.

Verify installation by calibrating the probe using the supplied calibration macros. If calibration macros are not supplied (such as Wilcox macros), run a calibration using PC-DMIS.

Updates to the Renishaw macros have been made for optimum ball-center probing. If, prior to a probing cycle, your probe drops in the Z axis by the probe's diameter, contact Renishaw for an update.

Next Step...