miim

### MP-048 TempComp or Laser system configuration error

Temperature Compensation configuration is incomplete, wrong, or inconsistent. Possible causes are:

- X, Y, or Z temperature inputs are not defined.

- No part thermistors have been defined.

- No probe thermistors have been defined.

- Pressure or humidity inputs have not been defined on a laser system.

- An internal inconsistency exists in the configuration data (e.g., a reference to a nonexistent thermistor).

What you should do:

1. To clear the error, click Clear error in the XYZ Display window.

To clear it using an RCU-II, press and hold down the Servo Power Off button and then press the Joy button twice.

2. If the error reoccurs, attempt to correct the problem by restoring the system configuration data from either the CONFG diskette or a saved host file.

3. If the error reoccurs, contact your Giddings & Lewis service representative.