laser

#### Feature Properties Area

XYZ Center or Point - These boxes show the feature’s XYZ center or point location in part coordinates.

IJK Surface, Edge, Slot, or Gap Dir (Vector) - These boxes allow you to set the surface normal vector, edge vector, slot vector, or gap direction of the feature.

IJK Angle Vector - These boxes allow you to define the feature's secondary vector. This helps control the orientation of the feature.

Polar/Cartesian Toggle - This button toggles the display between polar and Cartesian modes.

Find Nearest CAD - When you select an axis (X,Y, or Z) from one of the Center boxes and click this button, PC-DMIS finds the closest CAD element in the Graphic Display window to that axis.

Point Read From Machine - When you click this button, PC-DMIS uses the XYZ location of the machine for the feature’s XYZ coordinates.

Find Vector(s) - This button pierces all surfaces along the XYZ point and IJK vector looking for the closest point. The surface normal vector is displayed as the IJK NOM VEC but the XYZ values do not change.

This option is only available for Surface and Edge Point features.

Flip Vector - This button flips the surface normal vector. For example, 0,0,1 would flip to 0,0,-1.

Thickness - This field (T) applies a thickness to the feature. You can specify whether to use actual or theoretical values and then enter the value for the thickness.

Swap Vectors - Clicking this button causes the current edge vector and surface vector to switch vectors with each other.

This option is only available for Edge Point features.

Measure Now - This toggle button determines whether or not PC-DMIS measures the feature when you click Create.

Re-Measure - This toggle button determines whether or not PC-DMIS automatically re-measures the feature a second time once the feature has been measured. It will use the measure values from the first measurement as the target locations for the second measurement.

This is only available for Circle, Cylinder, Square Slot, Round Slot, and Notch features, and you must be in DCC Mode.