core

#### Reference temperature boxes

The Reference temperature boxes contain the reference temperature from which temperature compensation adjustments need to be applied.

- The amount of correction to be applied is based on multiplying the material coefficient by the difference between the current and reference temperatures.
  Amount of Correction = Material coefficient x (Current temperature – Reference temperature)

- If the current temperature is the same as the reference temperature, the net effect is that no thermal compensation adjustment is applied.

- The value in these boxes is almost always 20 degrees C, or the Fahrenheit equivalent.