miim

### MLB-080 Improper probe installed

The function is not compatible with the type of probe installed; for example, a sweep function is not valid when a touch probe is installed. This error may also occur on a system with a probe changer if the system is powered up with a probe mounted or a probe is manually mounted when the system believes that no probe is installed.

As a result, the command is not executed.

What you should do:

1. Check the command's definition and correct the measurement routine.

2. Adjust the installed equipment to correct the problem.