miim

### MP-018 MP internal counter error

The low byte of one of the software X/Y/Z counters differs from the low byte of the corresponding hardware counter. This error indicates a probable CPU board failure, not a counter board failure.

For more information, see "MP Error Codes".

What you should do:

1. To clear the error, power the MP down.

2. Power the MP back up.

3. If the error reoccurs, contact your Giddings & Lewis service representative.