core

## Inserting Move Commands: Introduction

This chapter discusses the various move commands that you can place in your measurement routine. Move commands provide you with the ability to alter the movement of the probe between hits.

The main topics covered in this chapter reflect the move commands that you can insert from the Insert | Move submenu and any other move commands. These topics include:

- Inserting a Move Point Command

- Inserting a Move Increment Command

- Inserting a Clearance Plane

- Inserting a Move Clear Plane Command

- Inserting a Move Circular Command

- Inserting a Move Sync Command

- Inserting a Move Sweep Command

- Inserting a Move All Command

- Inserting a Move Rotary Table Command

- Inserting a Move Exclusion Zone Command

- Inserting Clearance Moves Automatically

- Inserting a Clear Point Move

- Inserting Clearance Moves with Collision Detection