core

#### IJK Edge Boxes

These boxes are only available for the Edge Point and Line features.

The IJK Edge boxes define the approach direction (vector) for the edge hit or for the points of an auto line. This is a user-supplied I, J, K measured vector. The I, J, K should always point away from the edge and be perpendicular to the edge that is being measured.

After you define a new value, PC-DMIS normalizes the vector, making its length one unit.

T List and Box

The T ("thickness") list and box enable you to select the thickness type (theoretical, actual, or no thickness). For more information, see "Use Thickness".

Icon | Description
| Swap Vectors
| Flip Vector
| Read Vector from Machine (for Edge Point)