miim

### MP-186 Invalid W-axis MEA data

MEA data has not been collected for this machine's W-axis or the W-axis MEA data in EEPROM has been corrupted.

What you should do:

1. To clear the error, click Clear error in the XYZ Display window.

To clear it using an RCU-II, press and hold down the Servo Power Off button and then press the Joy button twice.

2. Collect W-axis MEA data using AutoCal or reload the configuration data with the correct configuration information from the CONFG disk.

3. If the error reoccurs, contact your Giddings & Lewis service representative.