portable

### SMX Reset tab

Machine Options dialog box - Reset tab

Home - Aims the laser to the BirdBath position.

Machine or Part coord. - Defines the coordinate system to use. Select Machine if you are using machine coordinates or Part coord. if you are using part coordinates.

Aim - Aims the laser to a point. Select a point from the Reset Point list, and click the Aim button to move the laser to the specified point.

Add - Opens the Point dialog box to add a point to the list above. From the Point dialog box, provide a Title and the XYZ values, and click Create. The new point is added to the list. For example, you might have attached reflectors to positions on a car door. You could then name these positions Door1, Door2, Door3, etc.

Delete - Removes a selected point from the list above.

ADM

Interferometer Only - Uses the interferometer laser for distance measurements. When starting or re-starting a measurement, it is typically initialized from the BirdBath.

Use Default Reset - Moves the Laser Tracker to the current Reset Point position.

Interferometer Set by ADM - Uses the interferometer laser for distance measurements. If the target gets lost by the Laser Tracker, the ADM laser find it. Once the ADM laser locates and sets the distance to the target, the interferometer laser calculates all distance measurements.

ADM Only - The software calculates all distance measurements with the ADM laser. If the target gets lost by the Laser Tracker, the ADM laser finds it.

Set Default Reset - Defines the selected point from the list as the default reset point. This is the point the laser points to if the beam is broken with your reflector.

Delay Before Positioning - Defines the time in milliseconds before the laser tracker points to the next position.

Aim Laser To Next Point - The laser tracker moves to the next point after completion of the previous point.