miim

#### Rotary Table

EnableRtaryTableVarCsy = -1 : If 1 or 0, the I++ DME command EnableRotaryTableVarCsy(x) will be sent with 1 or 0. This setting is used to control if the Csy turns with the rotary table. -1 means do not send the command.

InvertRT = FALSE : If TRUE, this setting will invert the rotary table sign.

KeeptRtPositive = FALSE : If set to TRUE, this setting ensures the rotary table value is always positive when going to the server. For example, -90 is sent as 270 which may be required by some servers.

ReadsRTCSY - When UsesRT is set to TRUE, the ReadsRTCSY registry entry uses the GetCsyTransformation(RotaryTableFixCsy) function to read the XYZ / IJK rotary table position and populates the PC-DMIS Rotary Table Setup dialog box with these values. The default value is FALSE.

RtOffset = 0 : Offset added to Server reading, e.g. to align rotary table 0 to a machine axis. The offset can be set dynamically via a specific external automation program.

UsesRT = FALSE : If TRUE, this setting will enable the use of the rotary table.