miim

### Interface-Specific Options

To set the values for registry entries for the FDC-SLC interface, use the PC-DMIS Settings Editor.
Laser (CWS or TTL) require different setups. For CWS, you need to set these registry entries:

Registry Entry | Default Value | Settings Editor Section
CWSPresent | TRUE | FDC
Laser_Type | 2 | MSI

For TTL, you need to set these registry entries:

Registry Entry | Default Value | Settings Editor Section
FLSPresent | TRUE | FDC
Laser_Type | 1 | MSI

If you install a rotary table, you need to set these additional settings:

Registry Entry | Default Value | Settings Editor Section
EnableRotaryAbsolutePosition | TRUE | FDC
EnableRotaryClockMode | TRUE | FDC
SendHSSFullData | 2 | FDC
RotaryMinDelta | 0.05 | FDC
RotaryOffset | 0 | FDC
RotaryOffsetSpeed | 50 | FDC
RotaryTablePresent | TRUE | FDC