core

### Plus Tolerance for Runout Dimensions

The Plus box in the Total Runout or Circular Runout dialog box (Insert | Dimension | Runout | Total or Insert | Dimension | Runout | Circular) enables you to enter a tolerance value along the plus direction. This means that any runout that differs from your nominal or theoretical runout can still be a valid measurement as long as it falls within the tolerance range specified.