settingseditor

### DccMeasureOrder

This registry entry determines the order that sample hits are taken for an edge point.

Entry Name: DccMeasureOrder

Entry Type: Whole number that specifies the measure order. The default value is 0.

Value Key

Value | Measure Order | Description
0 | Surface | This measures the three hits, first on the surface, and then on the edge.
1 | Edge | This measures the two hits, first on the edge and then the surface.
2 | Both | This measures the surface, and then the edge, and then the surface again.