Collapse All Expand All

PC-DMIS 2019 R1 Object Library |
QualificationSettings Object Members
See Also Overview Send Topic Feedback | See Object Hierarchy Chart

PCDLRN ActiveX DLL : QualificationSettings Object

Glossary Item Box

# Public Methods

GetTool | This method returns a tool object.
SetTool | Required expression that evaluates to a QualificationSettings object.

# Public Properties

CreateReplaceMap | This determines whether or not a map should be created or replaced. Read/Write.
EndA | This determines the ending A angle to use during qualification.
EndAngle | This determines the End Angle to use on the qualification tool.
EndB | This determines the ending B angle to use during qualification.
EndC | C Angle End Value
ExecuteMode | This determines the type of calibration action to take.
IncrementA | This determines the angle increment to use for the A angle during qualification.
IncrementB | This determines the angle increment to for the B angle during qualification.
IncrementC | C Angle Increment Value
Mode | This determines the Calibration Mode. Either DCC or Manual.
MoveSpeed | This determines the speed the probe moves during calibration.
NumHits | This determines the number of hits to take around the calibration tool.
NumLevels | This determines the number of levels that to use in the calibration process. PC-DMIS divides the number of hits by the number of levels to determine how many hits will be taken on each level of the qualification tool.
PHSAPriority | This indicates whether angle A or B for a PHS system receives priority during the calibration process. TRUE means Angle A gets priority. FALSE means Angle B gets priority.
PHSTol | For PHS systems, this determines the PHS tolerance value.
PreHit | This determines the Prehit distance to use during calibration.
ShankCheck | This determines whether or not you'll calibrate the shank of the probe as well.
ShankHits | This determines the number of hits used to measure the shank.
ShankOffset | Shank Offset for calibration
StartA | This determines the starting A angle to use during qualification.
StartAngle | This determines the Start Angle to use on the qualification tool.
StartB | This determines the starting B angle to use during qualification.
StartC | C Angle Start Value
ToolMoved | This indicates whether a tool has moved or not or if the user should be asked.
ToolOnRotaryTable | This indicates whether or not the tool is located on a rotary table.
ToolOverideI | This determines the I value for the Tool Override's IJK vector.
ToolOverideJ | This determines the J value for the Tool Override's IJK vector.
ToolOverideK | This determines the K value for the Tool Override's IJK vector.
Touchspeed | This determines the Touch Speed to use during calibration.
UserDefinedCalibrationMode | This determines whether End Angle, Start Angle, and NumLevels are used in the calibration process, or if they're ignored.
UserDefinedCalibrationOrder | This determines whether or not the calibration order is user defined.

# See Also

QualificationSettings Object

Copyright © 2019. Hexagon Manufacturing Intelligence – Metrology Software, Inc. All Rights Reserved.