portable

## Total Station Interface

To configure the parameters that control how PC-DMIS interfaces with the Total Station interface, select the Edit | Preferences | Machine Interface Setup menu item. This opens the Machine Options dialog box. The following tabs are available:

- Instrument Information tab

- Comm tab

- Reset Options tab

- Instrument Options tab

- Environmental Parameters tab

- Debug tab

Please refer to the your machine interface documentation for details.

### Instrument Information tab

Measurement Options dialog box - Instrument Information tab

### Comm tab

Measurement Options dialog box - Comm tab

### Reset Options tab

Measurement Options dialog box - Reset Options tab

On Break

This area lets you determine what happens when the laser beam from the Total Station to the probe is broken.

- Turn on laser pointer - This option turns on the laser pointer. For more information on the laser pointer, see the Laser Pointer ON/OFF menu item discussed in the "Total Station Menu" topic.

### Instrument Options tab

Measurement Options dialog box - Instrument Options tab

### Environmental Parameters tab

Measurement Options dialog box - Environmental Parameters tab

### Debug tab

Measurement Options dialog box - Debug tab

For information, see the "Generating a Debug File" topic in the "Setting Your Preferences" chapter in the PC-DMIS Core documentation.