laser

#### Sensor Frequency

This parameter controls the internal sensor frequency of the probe. The value that appears is the sensor pulses per second. For sensors with variable frequency capabilities, the higher the frequency, the more data you get. It is important to understand that more data is not always better. With variable frequency scanners, you should use a frequency in the middle of the supported range. This is a good balance between speed and accuracy.