core

Step 7 - Remove the Setting Gauge and Reconnect the Probe Assembly

For the ACR3 Probe Changer, after you have used the setting gauge to take the first (top face) hit and second (front edge) hit, do the following:

1. Remove the setting gauge from port 1 when you are prompted, as shown below:

PC-DMIS Message

Move the probe head clear of the ACR3.

Remove the setting gauge from port 1.

Reconnect the probe assembly.

The autojoint locking cam should be left backed off 5 degrees from the fully locked position.

After the probe assembly is reconnected, click OK.

Prompt for removing the setting gauge

2. Reconnect the probe assembly to the Autojoint to prepare for the remaining calibration as the message instructs.

3. After you have reconnected the probe assembly, click OK.

In the next step, you take the first manual probe hit.