miim

#### Scanning

AskForQ() = FALSE - Asks that the Q() parameter be returned with scan data. This Q() data is not used by PC-DMIS. Set to TRUE if a given server is "hard-wired" to transmit it.

MaxCommandLength - This is used as a check by the ScanOnCurve I++ command (any defined path scan) only. The default value is 65500 (64KB).

NoScan = FALSE - If TRUE, will prevent setting up the scan parameters // OBSOLETE

NonPlanarCircleScan - Forces PC-DMIS to generate the basic Circle scan (ScanOnCircle) instead of the Plane scan (ScanInPlaneEndIsPlane). The default value is TRUE.

ScanSpeed = 50 - Establishes a default speed for scanning commands.

ScansWillReportIJK = FALSE - If TRUE, PC-DMIS will prompt you if the scan report should include the IJK values.

ScansWillReportR = TRUE - If TRUE, will ask that the effective probe radius be transmitted back for scans.