core

#### Step 1 - Select the SP600 Probe Changer

To select the SP600 Probe Changer:

1. Select the Type tab in the Probe Changer dialog box (Edit | Preferences | Probe Changer).

Probe Changer dialog box - Type tab

2. To make this probe changer active and load the settings that are relevant to this probe changer, click Apply. Other tabs become visible after you click Apply.

3. In the Number of probe changers box, specify the number of different types of probe changers.

4. In the Active probe changer box, select the list item that represents the probe changer to define. If this is the first probe changer, it appears as Probe Changer 1: TYPE=None.

5. In the Probe changer type list, select SP600.

6. In the Docking speed box, type a value. The default value of 5% is appropriate for most machine configurations.

In the next step, you define the location your probe body moves to when using the probe changer to switch probe components.