miim

### Installation Information

The DLL for the Leitz interface is named LEITZ.DLL.

The PC-DMIS Settings Editor section headings for registry entries are:

- For most registry entries - LEITZ and USER_LEITZ

- For a small number of registry entries - Option and CMMAccuracy

You can use the Leitz interface on most of the controllers that use the Leitz protocol. These controllers include:

- Brown & Sharpe/DEA controllers (such as the Sharpe 32Z in Leitz mode and the Common Firmware controllers)

- Actual Leitz machines from Wetzlar

This interface is not intended for use on the Firmware Distributed Controller (FDC). FDC has a separate interface. For details, see "FDC Interface".

Some of the supported controllers communicate through a serial port, some use TCP/IP, and some support both methods according to how the controller is configured. This interface supports either method. You must configure the method to match how the controller is configured.