core

### Active Tip List

(This item pertains to the Probe Utilities dialog box, accessible through Insert | Hardware Definition | Probe.)

PC-DMIS is capable of storing data that describes a large number of probe tips. This data includes the probe tip's ID, rotation, type, location, direction, diameter and thickness, date and time of calibration, and any noncalibrated tips. These are all stored inside the Active Tip List.

Active Tip List

There can be as many as 32767 probe tips stored. This number may be limited by the amount of disk space available on your system.

PC-DMIS describes a probe according to the following criteria:

Tip List Description

1. TIP ID#This ID is the permanent number that PC-DMIS assigns to a tip when it is loaded into memory.
2. Tip Rotation This field displays the rotation of the tip in the vertical (A) and horizontal (B) direction
3. Tip Type This field displays the probe type (BALL, DISK, TAPER, SHANK, OPTICAL).
4. X,Y,Z Location These values describe the location of the tip. This location is in relation to the bottom of the Z rail.
5. I,J,K Direction These values describe the direction of the probe tip. This vector goes from the center of the probe tip towards the Z rail.
6. Diameter and Thickness These values describe the diameter of the tip and the thickness of SHANK and DISK probes. PC-DMIS defines these values when the probe is loaded. (To change a field see "Edit Tool".)
7. Date and Time These boxes indicate the most recent date and time the probe tip was calibrated. If a new tip is created without being calibrated, PC-DMIS will display "NEW" for the date and time values. If an old probe tip is loaded and the date and time information is unavailable, PC-DMIS will display "UNKNOWN" for the values. Only probe tips that are actually calibrated have their time and date values updated.

* (asterisk) - Noncalibrated Tip

An asterisk (*) to the left of the tip identifies any noncalibrated tips.

Adding Tips to the List

You can define new tips, adding them to the list, by using the Add Angles button. See the "Add Angles" topic.

Editing Tip Data

1. Highlight the desired active tip in the Active Tip List.

2. Press the Edit button.

An Edit dialog box appears, allowing you to change the displayed values.

Non-calibrated tips have an asterisk before their Tip ID # in the Active Tip List.

Setting the Calibration Order

The calibration order is determined by the order in which the tips are chosen from the list box.

To set the calibration order:

1. Select the User Defined option in the Measure Probe dialog box (See the "Measure" topic).

2. Hold down the Ctrl key on the keyboard.

3. With your left mouse button, select the tips from the Active Tip List for calibration. A number representing the index of the tip measurement order appears next to each Tip ID as it is selected.

If no tips are chosen, PC-DMIS prompts if you want to measure all tips.

Selecting a Tip to Use

You can define a specific probe tip to use in your measurement routine in these ways:

- Type TIP in the Edit window's Command mode and press the Tab key on your keyboard.

- Select the probe tip from the list on the Settings toolbar.

The Edit window command line for a sample tip would read:
TIP/T1A0B0, SHANKIJK=0, 0, 1, ANGLE=0

Until PC-DMIS encounters another TIP command in the measurement routine flow, it uses that tip.

Deleting a Tip or Wrist Angle

To delete one or more as tip from the Active Tip List:

1. Select the item or items to be removed.

2. Click the Delete button.

PC-DMIS also allows specific wrist angles to be removed from the Active Tip List. If a tip or probe head is deleted, all related wrist angles are also deleted from the file.

This option deletes the tip from the Active Tip List and removes it from the file of tips known to the system.