core

#### Calibrating the HR-MP (used with TM or THD) Probe Changer

This section describes how to calibrate the HR-MP (used with TM or THD) Probe Changer. The process discussed here is specific to the HR-MP (used with TM or THD) Probe Changer.

You can calibrate the probe changer in the following ways::

- When you calibrate the probe changer for the first time, you need to take the manual hits.

- When the probe changer is removed and mounted at the same location, you can select to calibrate the probe changer in DCC mode without taking manual hits.

- When the probe changer is removed and relocated on the CMM table, you can follow the same steps when you calibrate for the first time.

- The calibration of a single port is available in DCC or Manual mode.

To calibrate your probe changer:

Step 1 - Select the HR-MP Probe Changer

Step 2 - Define the Mount Point

Step 3 - Define the Number of Ports

Step 4 - Prepare for Calibration

Step 5 - Take the Manual Hits

Step 6 - Take the Manual Hit on Top of the Probe Support Tab

Step 7 - Review the Calibration Results

Recalibrate the Ports