miim

### Installation Information

Install PC-DMIS with a portlock or the LMS license correctly configured for the Metronics interface. This ensures that the correct files and registry entries are set up during the installation.

The license requires the following:

- Vision - Enabled

- Interface - Vision

- Vision Type - Metronics DCC / Metronics Manual (as required)

Additional requirements:

- Vision Frame Grabber should already be installed. For details, see "PC-DMIS Vision Frame Grabber and Camera Setup".