core

### Default (I,J,K, T) RMEAS Mode

When an Auto Feature has a relative planar measure feature associated with it (see "Relative To"), PC-DMIS measures the Auto Feature in a location that is adjusted according to the following rules:

- The measuring orientation of the Auto Feature is corrected by the rotation offset that exists between the orientation of the nominal and the actual RMEAS feature.

- The measuring location of the Auto Feature is corrected by the positional offset that exists between the location of the nominal and the actual RMEAS feature.

The Edit window command for this option is:

RMEAS/DEFAULT (I,J,K, T)

More:

Setting Up Relative Measure (RMEAS)

Math Process of the Default (I,J,K, T) RMEAS Mode