core

#### Auto Continue Execution if FindHole Fails

(This item pertains to the check boxes on the General tab of the Setup Options dialog box. You can open it through the F5 key or through the Edit | Preferences | Setup menu option.)

If you select the Auto Continue Execution if FindHole Fails check box, PC-DMIS allows you to automatically continue executing a part if the Find Hole option found on the Auto Feature dialog box fails to find a hole.

In the past, when the Find Hole option failed, PC-DMIS prompted you to place the probe in the center of the hole to continue running the measurement routine. However, with the Auto Continue Execution if FindHole Fails check box selected, PC-DMIS automatically prints an error message to the report and continues running the remaining measurement routine.

For more specific information on Find Hole, see the "Working with Contact Find Hole Properties" topic in the "PC-DMIS CMM" documentation.