core

#### Measuring a Round Slot

then | You can use these Round Slot icons to create a measured round slot.
To create a measured round slot, you must take at least six hits on the slot, usually two points on each straight side and one point on each curve. Alternately, you could take three points on each curve.
Example Round Slot with Six Points You can also create measured slots from two points. This is useful when the probe sphere is larger than the slot's diameter, and you're not able to take the required hits. For more information, see the PC-DMIS Portable documentation.
For information on the associated Edit window command, see the "Basic Measurement Format for a Round Slot" topic in the "Creating Measured Features" chapter.