miim

#### IDS Framegrabber

Test the IDS frame grabbers with the IdsDemo.exe application installed in \Program Files\IDS\FALCON\Samples folder by the IDS installer.

1. Run the IdsDemo application.

2. Click the FALCON | EAGLE menu item and select Initialize.

3. The video format defaults to PAL. If using NTSC, click the Properties button in the toolbar, then select the Video format tab, and select NTSC.

4. Select the Video Input button on the toolbar corresponding to the connected camera (the composite 3 button is selected in the picture below) and you should see a live camera image. Note this image is from a monochrome CCIR camera connected to an IDS Eagle.