miim

## Sheffield DCC

TNT and PCiia card settings

GPIB0

Bus Timing 500ns

Cable length for high speed disabled

Primary Address 0

Secondary Address None

Terminate read on EOS Yes

Set EOI with EOS on write Yes

8 bit EOS compare No

Send EOI at end of write Yes

EOS byte 3

System Controller Yes

I/O Timeout 10 sec

Parallel Poll duration default

Enable Auto Serial Poll Yes

Enable CIC Protocol No

Assert REN when SC No

CNTRLW

Primary Address 9

Secondary Address None

Terminate read on EOS Yes

Set EOI with EOS on write Yes

8 bit EOS compare No

Send EOI at end of write Yes

EOS byte 3

I/O Timeout 3 secs

Serial Poll Timeout 3 msec

Enable Repeat Addressing Yes

CNTRLR

Primary Address 8

Secondary Address None

Terminate read on EOS Yes

Set EOI with EOS on write No

8 bit EOS compare No

Send EOI at end of write No

EOS byte 3

I/O Timeout 3 secs

Serial Poll Timeout 1 sec

Enable Repeat Addressing Yes