core

Step 6 - Take the Second Manual Hit

You will take the second manual hit for the TESASTAR-PR / HR-P Probe Changer on the front face to the right of the last port. Once the first manual hit is completed, the following message box appears:

PC-DMIS Message

Please take a hit on the silver front face to the right of port 6.

Prompt for the second manual hit inside the last port

Use your machine's jog box to measure the second hit on the front surface to the right of the last port.

Location of second manual hit during calibration

WARNING: When you do this, the machine moves. To avoid injury, stay clear of the machine. To avoid hardware damage, run the machine at a slower speed.

After it takes this hit on the back of the last port, PC-DMIS drives in DCC mode and takes some additional measurements working backwards from the last port towards the first port. When this is complete, it positions the probe above the rack and provides instructions to proceed.

In the next step, you take the third manual hit.