miim

### MP-160 DCC board inoperative

On an MP-30, the DCC board failed its startup diagnostics.

On an SMP-400, the DCC board was not present though the SMP-400 was configured for DCC operations or the DCC board failed to function properly. In the latter case, a previous error report defined the cause of the failure.

For more information, see "DCC Error Codes".

What you should do:

1. To clear the error, power the MP down.

2. Power the MP back up.

3. Use the configuration data program to configure the MP correctly.

4. If the error reoccurs, contact your Giddings & Lewis service representative.