laser

#### Cylinder Command Mode Text

Sample Cylinder

CYL1 =FEAT/LASER/CYLINDER/DEFAULT,CARTESIAN,OUT

THEO/<3.1425,2.7539,0>,<0,0,1>,0.25,0.25

ACTL/<3.1425,2.7539,0>,<0,0,1>,0.25,0.25

TARG/<3.1425,2.7539,0>,<0,0,1>

DEPTH=0

CENTER OFFSET=0

SEARCH LENGTH=0

SHOW FEATURE PARAMETERS=NO

SHOW_LASER_PARAMETERS=YES

POINT CLOUD ID=COP1

HORIZONTAL CLIPPING=0.0787,VERTICAL CLIPPING=0.0787

RINGBAND=ON,INNER OFFSET=0.5,OUTER OFFSET=2

More:

Laser Cylinder

Cylinder Specific Parameters

Auto Cylinder Paths