core

Step 1 - Select the TESASTAR-PR / HR-P Probe Changer

To select the TESASTAR-PR / HR-P Probe Changer:

1. Select the Type tab in the Probe Changer dialog box (Edit | Preferences | Probe Changer).

2. In the Probe changer type list, select TESASTAR-PR / HR-P:

Probe Changer dialog box - Type tab

3. To make this probe changer active and to load settings that are relevant to it, click Apply. Other tabs become visible after you click Apply.

4. In the Active probe changer box, select the list item that represents the probe changer you want to define. If this is the first probe changer, it appears as Probe Changer 1: TYPE=None.

5. In the Number of probe changers box, specify the number of probe changers that you want to define.

6. In the Docking speed box, type a value. 15% is appropriate for this machine configuration.

In the next step, you define the mount point and wrist angles for your system.