cmm

#### Enter DCC Mode

This step adds a command that executes commands below it in Direct Computer Control (DCC) mode. In DCC mode, your computer controls the motions of the CMM.

1. In the Edit window, place your cursor after the end of the A1 alignment command block.

2. From the Probe Mode toolbar, click the DCC Mode button ().

3. PC-DMIS inserts a MODE/DCC command into the Edit window after the ALIGNMENT/END command. When you execute, PC-DMIS executes commands after this in DCC mode.

For more information about the CMM modes, see "Probe Mode Toolbar" in the "Using Toolbars" chapter.