miim

#### Assignment of Keys

You can find the "P" button just above the jog box joystick. Depending on the setting of the UsePButton and UseSendKey registry entries in the registry, you are able to assign the "P" button and the "Send" key.

This assignment assumes that the settings in the CEJComm.ini file are correct.

For details on assigning buttons and keys, see the "Assignment of Keys" topic.