miim

### Troubleshooting Tips

Problem | Cause | Solution
The machine immediately shakes when it tries to move. | The YY settings may be bad. |
Motion starts, but then a motion error occurs. | The acceleration or velocity settings may be bad. | Try to disable axis optimization (AO).
A "CMM not responding" error occurs. | Open Windows Task Manager to see if a second PC-DMIS application (pcdlrn.exe) is running. |
There are long delays before measurements. | SERL may be set as too precise. | Increase the number.
There are only readouts, and hits do not register. | Set the SETPT registry entry to TRUE. This registry entry is in the USER_LK section of PC-DMIS Settings Editor. |
The machine does not home. | This be due to a PDAMP command in your DOWNL.OAD file. | Use a "!" to comment out the command.
Most LKs in version 2.21 do not successfully initialize. | Version 2.21 has a known problem. For more information, see "Updates". | Upgrade the software.

For the LK-2000 to display updated scales with joystick motion, PC-DMIS must be in Readouts mode. To select this mode, click the Readouts Mode icon on the Probe Mode toolbar in PC-DMIS. The icon is also located in the Probe Toolbox in the Auto Feature dialog box.

To take a manual hit, select the Hits Mode icon on the Probe Mode toolbar to return to Hits mode.