planner

Step 1 - Select the I++ Client Probe Changer

To select the I++ Client Probe Changer:

1. Select the Type tab in the Probe Changer dialog box (Edit | Preferences | Probe Changer):

Probe Changer dialog box - Type tab

2. To make this probe changer active and to load the settings that are relevant to it, click Apply.

3. Ensure that the value of "1" appears in the Number of probe changers box.

4. In the Probe changer type list, select I++ Client.

5. Click Apply.

6. In the Active probe changer box, select TYPE=IPlusPlus-Client

7. Note that you cannot change the value that appears in the Docking speed box.

In the next step, you assign the probes to the port.