portable

## Finding a Reflector

The Find function allows you to search in a spiral pattern to find the actual location of a reflector or T-Probe (6dof system only) with your Leica Tracker or Total Station device.

Finding a Reflector Location Using a Leica Tracker Device

1. Point the Tracker laser approximately to the location of the desired reflector. You can do this in these ways:

- "Releasing Tracker Motors" (6dof system only) and manually moving the laser to the location.

You do not need to release the motors on the 3D systems.

- Use the control buttons on the ADM tab of the Machine Options dialog box (Edit | Preferences | Machine Interface Setup).

- Use the Overview camera.

- Use the Alt + left arrow, right arrow, up arrow, and down arrow keyboard keys to move the tracker head. Use Alt + Space to stop movement of the laser.

2. Select the Tracker | Find menu item. The tracker device searches in a spiral pattern and take readings until the reflector sends the signal back to the device. This locates the position.

Finding a Reflector Location Using a Total Station Device

1. Point the Total Station laser approximately to the location of the desired reflector. You can do this in these ways:

   - Manually move the laser to the location.

   - Use the Alt + left arrow, right arrow, up arrow, and down arrow keyboard keys to move the tracker head. Use Alt + Space to stop movement of the laser.

2. Select the Total Station | Find menu item. The total station device searches in a spiral pattern and takes readings until the reflector sends the signal back to the device. This locates the position.

You can only execute this function from the View Camera dialog box.