core

#### Arm1 Probe File Calibration

If you want to calibrate the Arm1 probe file:

1. Select the Arm 1 Active icon from the Active Arms toolbar (View | Toolbars | Active Arms).

2. Access the Probe Utilities dialog box (Insert | Hardware Definition | Probe).

3. Follow existing procedures in the "Calibrating Probe Tips" topic of the "PC-DMIS CMM" documentation for information on how to calibrate probe files.